PRESS ENERGY SERVICES SAFETY COURSES

“VACUUM TRUCK TRANSPORT”

1. CHECKING IN WITH DISPATCH, VERIFYING THE SPECIFIC LOCATION AND ROUTE TO SITE, KNOWING WHAT TYPE OF VOLUME OF FLUID IS BEING HAULED ARE ALL PART OF?:

A. PLANNING YOUR TRIP.

B. STATE REGULATIONS.

C. BEING STREET SMART

D. ARRIVAL AND TRANSFER.

1. CARRIERS MUST TRANSPORT FLUIDS TO PRODUCTION COMPANIES APPROVED SITES?

A. TRUE B. FALSE

3. WHICH OF THE FOLLOWING IS REQUIRED EQUIPMENT?

A. TIRE CHOCKS

B. ORANGE REFLECTIVE SAFETY CONES

C. PARTICLE SCREENS

D. ALL OF THE ABOVE.

4. WHEN DO YOU HAVE TO CHECK IN WITH THE COMPANY MAN OR FLOWBACK HAND?

A. UPON ARRIVING AT THE SITE

B. BEFORE DEPARTING THE SITE

C. BOTH A AND B

D. ALL OF THE ABOVE

5. MAXIMUM SPEED LIMIT ON LEASE ROADS IS\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_AND\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ON THE PAD.

A. 20 MPH, 15 MPH

B. 10 MPH, 5 MPH

C. 5 MPH, 35 MPH

D. 15 MPH, 5 MPH

6. TRUCKS SHOULD BE PLACED NO CLOSER THAN \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ FROM THE EDGE OF A PIT OR POND.

A. 3 FEET

B. 5 FEET

C. 6 FEET

D. 10 FEET

7. WHICH OF THE FOLLOWING IS TRUE ABOUT SHALLOW GROUND WATER?

A. IT IS RECOVERED FROM SHALLOW FORMATIONS DURING THE AIR DRILLING PROCESS.

B. IT IS KNOWN AS OILY WATER

C. IT CAN BE RECYCLED

D. BOTH A AND C

8. YOU MUST USE A SCREEN FITTING ON THE HOSE, PLACE A FLOAT ON THE HOSE AND TAPE DOWN THE CAMLOCK EARS TO PREVENT THEM FROM DRAGGING ON THE BOTTOM OF THE PIT AND POSSIBLY TEARING THE LINER?

A. TRUE

B. FALSE

9. PPE IS DESIGNED TO PROTECT WORKERS FROM SERIOUS WORKPLACE INJURIES?

A. TRUE

B. FALSE

10. WHEN TRANSFERRING ON ACTIVE SITES WHAT ARE SOME ADDITIONAL MEASURES YOU MUST TAKE TO PREVENT LEAKS?

A. GROUND BARRIERS MUST BE IN PLACE

B. SPILL PROTECTION AND BERMS MUST BE IN PLACE

C. PLACE OIL ABSORBENT PADS UNDER HOSE CONNECTIONS

D. ALL OF THE ABOVE